Diagram

Description automatically generated

Figure 2‑5. The experimental setup for GRID irradiation of gafchromic films. For calibration, no GRID was used.